reference | 9.06.2016 08.44

Building | Design Heat Loss, W | Rotation, deg | Net - Gross Volume, m³
--- | --- | --- | ---
Jagtvej 110 |  | 330 | 272,85 | 374,395
Site | Weather File | Ground | Terrain Type
| Copenhagen | CPH.DRY |  | City

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
A TH ThermalZone |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
ATH |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 600 mm (Ydervæg) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,6 0,24 0,24 0,24 0,24 0,24 | 0,429401 0,429401 1,00471 1,69456 1,69456 1,69456 1,69456 1,69456 | 20,1939 20,1939 6,5328 12,2 9,98057 3,1598 1,38027 3,11303 | 24,4688 24,4688 8,6444 15,9588 13,2385 3,94785 2,08536 3,94185
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Dannebrog Reference Interior door, wood Interior door, wood | 330 101,228 150 | 4,15068 1,50805 1,50805 | 2,12 0 0 | 3,52 1,68001 1,68
Systems | Component | Control | Time
Equipment | Intern Belastning | FullLoad | Always
Infiltration | Naturlig Ventilation 0,4 /h. | FullLoad | Always
Heating | Opvarmning | HeatCtrlDay | HeatingSeason
Venting | Venting 0,4 /h Max: 1,2 /h | VentingCtrl 23 C | Maj-Sept 07 - 22

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
A TV ThermalZone |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
ATV |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 600 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,24 0,6 0,24 0,24 0,24 0,24 | 0,429401 0,429401 1,69456 1,00471 1,69456 1,69456 1,69456 1,69456 | 20,1939 20,1939 12,2 6,5328 9,98057 3,4318 1,38027 2,84103 | 24,4688 24,4688 15,9588 8,6444 13,2386 4,49985 2,08536 3,38985
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Dannebrog 1100 mm (Type A) Interior door, wood Interior door, wood | 330 150 198,772 | 5,98409 1,50805 1,50805 | 3,52 0 0 | 3,52 1,68 1,68001
Systems | Component | Control | Time
Equipment | Intern Belastning | FullLoad | Always
Infiltration | Naturlig Ventilation 0,4 /h. | FullLoad | Always
Heating | Opvarmning | HeatCtrlDay | HeatingSeason
Venting | Venting 0,4 /h Max: 1,2 /h | VentingCtrl 23 C | Maj-Sept 07 - 22

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
Øvrige - ThermalZone |  | 71,7522 | 85,2542 | 174,303 | 237,859
Øvrige rum |  | 71,7522 | 85,2542 | 174,303 | 237,859
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 600 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,24 0,24 0,24 0,6 0,35 0,35 0,24 0,24 0,24 0,6 0,35 0,35 0,24 0,6 0,35 0,35 0,6 0,24 0,24 | 0,429401 0,429401 1,69456 1,69456 1,69456 1,00471 0,429401 0,429401 1,69456 1,69456 1,69456 1,00471 0,429401 0,429401 1,69456 1,00471 0,429401 0,454789 1,00471 1,69456 1,69456 | 15,5153 15,576 11,3948 3,4318 3,08817 6,56048 15,576 15,576 11,3948 3,1598 3,36017 6,56049 31,8678 31,8072 3,69149 14,9271 8,79313 8,80096 3,0418 9,87957 9,87957 | 18,3574 18,3574 15,0381 4,49985 3,38985 6,43774 18,3574 18,3574 15,0381 3,94785 3,94185 6,43775 37,3413 37,3413 4,17073 19,6371 11,1982 11,1982 4,8244 13,2385 13,2386
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Interior door, wood Dannebrog Reference Interior door, wood Interior door, wood Dannebrog Reference Dannebrog Reference Dannebrog Reference | 330 150 281,228 18,772 221,758 78,2424 330 | 1,50805 4,24746 1,50805 1,50805 4,20691 4,20691 3,99318 | 0 2,39999 0 0 1,2 1,2 0,9984 | 3,36 3,84001 1,68001 1,68001 1,94752 1,94752 1,76
Systems | Component | Control | Time
Heating | Opvarmning | HeatCtrlDay | HeatingSeason