150cm | 9.06.2016 17.28

Building | Design Heat Loss, W | Rotation, deg | Net - Gross Volume, m³
--- | --- | --- | ---
Jagtvej 110 |  | 180 | 272,85 | 374,395
Site | Weather File | Ground | Terrain Type
| Copenhagen | CPH.DRY |  | City

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
A TH ThermalZone |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
ATH |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 600 mm (Ydervæg) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,6 0,24 0,24 0,24 0,24 0,24 | 0,429401 0,429401 1,00471 1,69456 1,69456 1,69456 1,69456 1,69456 | 20,1939 20,1939 4,6848 12,2 9,98057 3,1598 1,38027 3,11303 | 24,4688 24,4688 6,7964 15,9588 13,2385 3,94785 2,08536 3,94185
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Glasdør Type A Glasdør Type A Interior door, wood Interior door, wood | 180 180 311,228 0 | 1,51069 1,51069 1,50805 1,50805 | 1,69 1,69 0 0 | 2,684 2,684 1,68001 1,68
Systems | Component | Control | Time
Equipment | Intern Belastning | FullLoad | Always
Infiltration | Naturlig Ventilation 0,4 /h. | FullLoad | Always
Heating | Opvarmning | HeatCtrlDay | HeatingSeason
Venting | Venting 0,4 /h Max: 1,2 /h | VentingCtrl 23 C | Maj-Sept 07 - 22

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
A TV ThermalZone |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
ATV |  | 20,1939 | 24,4688 | 49,2732 | 68,2681
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 600 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,24 0,6 0,24 0,24 0,24 0,24 | 0,429401 0,429401 1,69456 1,00471 1,69456 1,69456 1,69456 1,69456 | 20,1939 20,1939 12,2 4,6848 9,98057 3,4318 1,38027 2,84103 | 24,4688 24,4688 15,9588 6,7964 13,2386 4,49985 2,08536 3,38985
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Glasdør Type A Interior door, wood Interior door, wood | 180 0 48,772 | 1,73126 1,50805 1,50805 | 3,38 0 0 | 5,368 1,68 1,68001
Systems | Component | Control | Time
Equipment | Intern Belastning | FullLoad | Always
Infiltration | Naturlig Ventilation 0,4 /h. | FullLoad | Always
Heating | Opvarmning | HeatCtrlDay | HeatingSeason
Venting | Venting 0,4 /h Max: 1,2 /h | VentingCtrl 23 C | Maj-Sept 07 - 22

Thermal Zone | Design Heat Loss, W | Net - Gross Floor Area, m² | Net - Gross Volume, m³
--- | --- | --- | ---
Øvrige - ThermalZone |  | 71,7522 | 85,2542 | 174,303 | 237,859
Øvrige rum |  | 71,7522 | 85,2542 | 174,303 | 237,859
Enclosing Elements | Building Element | Thick, m - U, W/m² K | Net - Gross Area, m²
Constructions | Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 240 mm (Indervæg) Mursten 600 mm (Ydervæg) Gulv (Etageadskillelse) Loft (Etageadskillelse) Mursten 600 mm (Ydervæg) Mursten 240 mm (Indervæg) Mursten 240 mm (Indervæg) | 0,35 0,35 0,24 0,24 0,24 0,6 0,35 0,35 0,24 0,24 0,24 0,6 0,35 0,35 0,24 0,6 0,35 0,35 0,6 0,24 0,24 | 0,429401 0,429401 1,69456 1,69456 1,69456 1,00471 0,429401 0,429401 1,69456 1,69456 1,69456 1,00471 0,429401 0,429401 1,69456 1,00471 0,429401 0,454789 1,00471 1,69456 1,69456 | 15,5153 15,576 11,3948 3,4318 3,08817 6,56049 15,576 15,576 11,3948 3,1598 3,36017 6,56049 31,8678 31,8072 3,69149 14,9271 8,79313 8,80096 3,0418 9,87957 9,87957 | 18,3574 18,3574 15,0381 4,49985 3,38985 6,43775 18,3574 18,3574 15,0381 3,94785 3,94185 6,43775 37,3413 37,3413 4,17073 19,6371 11,1982 11,1982 4,8244 13,2385 13,2386
Enclosing Elements | Building Element | Orient, deg - U, W/m² K | Glass - Opening Area, m²
Windoors | Interior door, wood Dannebrog Reference Interior door, wood Interior door, wood Dannebrog Reference Dannebrog Reference Dannebrog Reference | 180 0 131,228 228,772 71,7576 288,242 180 | 1,50805 4,24745 1,50805 1,50805 4,20691 4,20691 3,99318 | 0 2,39998 0 0 1,2 1,2 0,9984 | 3,36 3,84 1,68001 1,68001 1,94752 1,94752 1,76
Systems | Component | Control | Time
Heating | Opvarmning | HeatCtrlDay | HeatingSeason